SW1

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

!

hostname SW1

!

!

!

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

interface FastEthernet0/1

switchport mode access

switchport port-security

switchport port-security mac-address sticky

switchport port-security mac-address sticky 000A.4183.7D42

!

interface FastEthernet0/2

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/3

switchport mode access

switchport port-security mac-address sticky

!

interface FastEthernet0/4

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/5

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/6

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/7

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/8

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/9

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/10

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/11

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/12

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/13

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/14

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/15

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/16

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/17

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/18

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/19

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/20

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/21

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/22

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/23

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface FastEthernet0/24

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface GigabitEthernet0/1

switchport mode access

!

interface GigabitEthernet0/2

switchport mode access

switchport port-security

switchport port-security mac-address sticky

shutdown

!

interface Vlan1

no ip address

shutdown

!

banner motd ^CSW1 - Unauthorized access prohibited^C

!

!

!

line con 0

!

line vty 0 4

login

line vty 5 15

login

!

!

!

!

End

R1

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

security passwords min-length 10

!

hostname R1

!

!

!

enable secret 5 $1$mERr$2kSZR9DN2ofxLllbGij.S1

!

!

!

!

!

aaa new-model

!

aaa authentication login RADIUS group radius local

aaa authentication login default local

!

!

!

!

!

!

!

ip cef

no ipv6 cef

!

!

!

username user secret 5 $1$mERr$2kSZR9DN2ofxLllbGij.S1

!

!

!

!

!

!

!

!

ip ssh version 2

ip domain-name domain

!

!

spanning-tree mode pvst

!

!

!

!

!

!

interface GigabitEthernet0/0/0

ip address 192.168.1.254 255.255.255.0

duplex auto

speed auto

!

interface GigabitEthernet0/0/1

no ip address

duplex auto

speed auto

shutdown

!

interface Vlan1

no ip address

shutdown

!

ip classless

!

ip flow-export version 9

!

!

!

banner motd ^CR1 - Unauthorized access prohibited^C

!

radius-server host 192.168.1.1 auth-port 1645 key aaa

!

!

!

!

line con 0

exec-timeout 5 0

login authentication tacacs

!

line aux 0

exec-timeout 5 0

!

line vty 0

exec-timeout 5 0

login authentication RADIUS

transport input ssh

line vty 1 4

exec-timeout 5 0

transport input ssh

line vty 5 15

exec-timeout 5 0

transport input ssh

!

!

!

End

SR1



