RouterA

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname RouterA

!

!

!

enable secret 5 $1$mERr$9cTjUIEqNGurQiFU.ZeCi1

!

!

ip dhcp excluded-address 192.168.10.1 192.168.10.10

!

ip dhcp pool VOICE

network 192.168.10.0 255.255.255.0

default-router 192.168.10.1

option 150 ip 192.168.10.1

!

!

!

ip cef

no ipv6 cef

!

!

!

!

!

!

!

!

!

!

no ip domain-lookup

!

!

spanning-tree mode pvst

!

!

!

!

!

!

interface FastEthernet0/0

ip address 192.168.10.1 255.255.255.0

duplex auto

speed auto

!

interface FastEthernet0/1

no ip address

duplex auto

speed auto

shutdown

!

interface Vlan1

no ip address

shutdown

!

ip classless

!

ip flow-export version 9

!

!

!

banner motd ^C

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

RouterA

Authorized Access ONLY

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

^C

!

!

!

!

!

telephony-service

max-ephones 5

max-dn 5

ip source-address 192.168.10.1 port 2000

auto assign 4 to 6

auto assign 1 to 5

!

ephone-dn 1

number 54001

!

ephone-dn 2

number 54002

!

ephone 1

device-security-mode none

mac-address 0090.0C04.809E

type 7960

button 1:1

!

ephone 2

device-security-mode none

mac-address 0001.4219.444A

type 7960

button 1:2

!

line con 0

password cisco

login

!

line aux 0

!

line vty 0

password cisco

login

line vty 1 4

login

!

!

!

End

SwitchA

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname SwitchA

!

enable secret 5 $1$mERr$9cTjUIEqNGurQiFU.ZeCi1

!

!

!

mls qos

!

no ip domain-lookup

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

interface FastEthernet0/1

switchport mode access

switchport voice vlan 1

mls qos trust cos

mls qos trust device cisco-phone

!

interface FastEthernet0/2

switchport mode access

switchport voice vlan 1

mls qos trust cos

mls qos trust device cisco-phone

!

interface FastEthernet0/3

switchport mode access

switchport voice vlan 1

mls qos trust cos

mls qos trust device cisco-phone

!

interface FastEthernet0/4

switchport mode access

switchport voice vlan 1

mls qos trust cos

mls qos trust device cisco-phone

!

interface FastEthernet0/5

switchport mode access

switchport voice vlan 1

mls qos trust cos

mls qos trust device cisco-phone

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface GigabitEthernet0/1

!

interface GigabitEthernet0/2

!

interface Vlan1

no ip address

shutdown

!

banner motd ^C

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SwitchA

Authorized Access ONLY

^C

!

!

!

line con 0

password cisco

login

!

line vty 0

password cisco

login

line vty 1 4

login

line vty 5 15

login

!

!

!

!

end